Q2N5109 Q1 Q2N5109 Q2 Q2N5109 Q3 Q2N5109 Q4

Q2N5109 Q5 Q2N5109 Q6 Q2N5109 Q7 Q2N5109 Q8

1 2 3 ZVN4206A M1 1 2 3 ZVN4206A M2

1 2 3 ZVN4206A M3 1 2 3 ZVN4206A M4

1

2 3 BAV99 D1 1

2 3 BAV99 D2 1

2 3 BAV99 D3 1

2 3 BAV99 D4

1

2 3 BAV99

D6 1

2 3 BAV99 D8

50 R1

50 R2 100n C1

500 R3 500 R4 500 R5 500 R6

100n C16 100n C2

330 R8

100n C4

43 R9 100n

C5 43R10

50 R11

100n C6

43 R13 100n C7 43 R14

43 R15 100n C8 43 R16

330 R17

100n C9

50 R19

50 R20

43 R21 100n C10 43 R22

50 R23 50 R24

100n C11

330 R26

500 R27 500 R28 500 R29 500 R30

50 R31

50 R32 100n C12

50 R33 330 R34 50 R35

50 R36 33 R7 33 R12

33 R25 33 R18 1

2 3 BAV99 D7

S1 5 D1 7 CE1 6 R1 4 C 9 R2 13 CE2 11 D2 10 S2 12

Q1 2 Q1 3

Q2 14

Q2 15

VCC1 1 VCC2 16

VEE 8 10130

U1

1

2 3 BAV99 D5

S1 5 D1 7 CE1 6 R1 4 C 9 R2 13 CE2 11 D2 10 S2 12

Q1 2 Q1 3

Q2 14

Q2 15

VCC1 1 VCC2 16

VEE 8 10130

U2 Clk_A_Out_p

Cmd_A_Out_n

Cmd_A_Out_p Cmd_B_Out_p

Cmd_B_Out_n

D5_Local

D0_Local

Clk_In_p

Clk_In_n

Cmd_In_p

Cmd_In_n

Reset_A Reset_B Enable_High_Current_A Enable_High_Current_B

Clk_A_Out_n Clk_B_Out_p Clk_B_Out_n

D0_Local

D5_Local

D5_Local

D5_Local

D5_Local D5_Local

D5_Local

D0_Local

D0_Local D0_Local

D0_Local

D0_Local

D5_Local

D0_Local

D0_Local D0_Local

D0_Local D0_Local

The drivers are intended to deliver output of 500 mVp-p at the ATOM chip inputs.

The 10130 dual D-Latch chips freeze the clock and command drivers in a low state when the Reset_A or B lines are high. This prevents

The Enable A and B lines reduce the drive current when drivers are not active. They are used with the signals from toggling while the ATOM chips are being powered up or when the channel is not selected for use.

the Select lines to present a fixed logic low signal to the ATOM chip inputs when the channel is not selected and when the ATOM chips are powered up. For D5 levels below 3V, the driver outputs are in an undefined low current state.

Clock A Cable Driver Clock B Cable Driver

Cable Driver

Command B Cable Driver

Command A

Bypass caps for U1 and U2.

PRELIMINARY

SCIPP Santa Cruz, CA 95064 408-459-2694

Revision: Page of

Page Size:

1.20 2/10/97

Cab_Drv,sch

B BABAR HDI Link Card

Clk/Cmd Cable Drivers

TITLEBLK_B

1 1