.225 in

1.33 in ( 3.4 cm )DetectorAssemblyboard

.20 in typ.

2.36 in ( 6 cm )

0.56 in SupportCardNote 3Ref.

5.70 in

1.242 in

1.802 inFlat Strain Relief

CoolingPipe

3-M 344350 pin Connector.50 in

.25 in

Note 1Alignment Edge

Alignment Edge

2.85 in Area For Cooling PipeNote 2Note 3Round Strain Relief

3.65 in 3.648 inKapton HybridDetector

1.12 in

.170 inNo comp. zone

0.56 in .372 in

3.33 in 3.35 in

.800 inKapton Width

.50 in(Det.Glue Joint toCenter Line of Kapton)

.50 inNote 4SurfaceMounts

2.09 inReference

5.12 in Reference

Note 1: Berg Electronics Surface-Mount Header # 87409-120 Berg Electronics Recepticle # 87815-620Note 2: Actual kapton length is 1.312 in. to connector center line which allows 0.070 in. flex of kapton for connector engagement.Note 3: These dimensions may be changed depending on final electronics layout.7/10/95Rev.SCIPP

Note 4: Power Connector. Dimensions to be determinedH8 BINARY READ-OUT DETECTOR ASSEMBLY (3.4 X 6)cm DETECTOR

7.00 in

1.55 in