COOLANT IN

Stainless steelBLOCK1x2x3,with BORE&FITTINGSfor COOLANT

V , i1411

PYROLYTICGRAPHITE12x6x1mnmwith 6x1 "EAR"possibly covered withCarbon-carbon sheet

??RTDLOCATION 52 56 89 15M-MODULE

SCIPPRev. 4/21/96